[SVSNET]
 Type       = NDIS
 Title      = "TAP Driver for Vbox/2"
 Version    = 1.00
 DriverName = TAP$
 Xports = NETBEUI LANDD

[File]
 Name     = Prot.OS2
 Path     = IBMCOM\MACS

[HandleArps]
  Display    = "Handle ARP"
  Type       = Decimal
  Range      = 0-1
  Default    = 1
  Optional   = Yes
  Editable   = Yes
  Help       = "No idea what this parameter does, so don't change it"

