[DC21X4]
Type = NDIS



Title = "Intel 2104x/2114x 10/100 mbps Ethernet Controller"


Version = 3.00
DriverName = DC21X4$
Xports = NETBEUI, LANDD

[FILE]
Name = DC21X4.OS2
Path = IBMCOM\MACS



[SLOT]
display = "Slot Number of the Adapter"
type = decimal
default = "16"
optional = yes
range = 16-26
help = "This parameter sets the slot number of the adapter.
For a PCI adapter, use 16 for the first adapter in the system,
17 for the second, and so on."

[ConnectionType]
display = "Connection Type"
type = string
strlength = 32
optional = yes
set = Autosense,_10Base2_(BNC),_10Base5_(AUI),_10BaseT,_10BaseT_FD,_10BaseT_No_Link_Test,_100BaseTx,_100BaseTx_FD,_100BaseT4
default = AutoSense
help = "This parameter specifies the connection type and line
speed, used on the adapter."
